Therometer Box: Front Panel

On

O f f

A B C D

Byp ass

In

Bypass: When the switch is "Bypass", then the resistor is having

current sent through it. The switch for this resistor is open.

In: When the switch is "In", then the resistor is n ot having

current sent through it. The switch for this resistor is open.

On/Off: This is the power switch. When the switch is "On", the

circuit is closed. When the switch is "Off", the circuit is open.

M. C. Herda

Univ of Md

May 28, 2000