G0 T arget Controls Status

E. Beise, Fall 99

Custom Hardware

· Target Heater suppl yoverride circuit (complete)

· 2 Oxford controllers in house (6 sensors) (tests underway)

· Vacuum Interlock box (to be designed)

· FSD Interlock box (to be designed)

· JT valve controller (JLAB)

· Pump controller (underway at Caltech)

· Connector specifications for Breakout Box

· All cabling still to be specified

EPICS-based controls software

· Specifications document mostlycomplete www2.physics.umd.edu/~beise/g0-exp/EPICS-specs.html

· S. W itherspoon of software division contacted, work begun

(Aug 99)

· EPICS software delivery(JLAB) added to W BS

· VME hardware purchase $ still to be identified

VME Hard ware Requirements for EPICS based system

Greenspring IPs (presentl yin use in Hall C)

Item number item cost net cost

VME crate 1 $2,478.00 $2,478.00

VME MV68040 IOC 1 $3,300.00 $3,300.00 transition module 1 $340.00 $340.00

VME Carrier Board 2 $510.00 $1,020.00

IPADIO (8 ADC, 68 dig I/O, 2 DAC) 4 $795.00 $3,180.00

IP quadrature (4 counter/timers) 1 $375.00 $375.00

Serial interface (IPoctal232) 1 $345.00 $345.00 relayVMIVME2232-100 (32) 1 $1,125.00 $1,125.00 total $12,163.00

Does not include spare parts